### Correct Data Set for Truck Inspection

\*\*Tire Pressure:\*\*

\* The correct tire pressure for the left front is 33-35 PSI.

\* The correct tire pressure for the right front is 33-35 PSI.

\* The correct tire pressure for the left rear is 33-35 PSI.

\* The correct tire pressure for the right rear is 33-35 PSI.

\*\*Battery Inspection:\*\*

\* The correct voltage range is 12.4-12.7 volts.

\* The correct water level is full.

\* There should be no visible damage, leaks, or rust.

\*\*Exterior Inspection:\*\*

\* There should be no signs of rust, dents, or damage.

\* There should be no oil leak in the suspension.

\*\*Brake Inspection:\*\*

\* The correct brake fluid level is full.

\* The front brakes should be in good condition.

\* The rear brakes should be in good condition.

\* The emergency brake should be in good condition.

\*\*Engine Inspection:\*\*

\* There should be no signs of rust, dents, or damage.

\* The engine oil should be in good condition and have a clean color.

\* The brake fluid should be in good condition and have a clean color.

\* There should be no oil leak in the engine.